<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="30" width="0" layer="20"/>
<wire x1="0" y1="30" x2="112" y2="30" width="0" layer="20"/>
<wire x1="112" y1="30" x2="112" y2="0" width="0" layer="20"/>
<wire x1="112" y1="0" x2="0" y2="0" width="0" layer="20"/>
<text>PCB Layers</text>
<text>Silkscreen</text>
<text>Soldermask</text>
<text>Top Copper</text>
<text>Substrate</text>
<text>No Layers</text>
<text>Silkscreen</text>
<text>Soldermask</text>
<text>Bottom Copper</text>
<text>Substrate</text>
<text>No Layers</text>
<text>PCB Layers</text>
<wire x1="11" y1="18" x2="21" y2="18" width="0" layer="46"/>
<wire x1="21" y1="18" x2="22" y2="17" width="0" layer="46" curve="-90"/>
<wire x1="22" y1="17" x2="22" y2="7" width="0" layer="46"/>
<wire x1="22" y1="7" x2="21" y2="6" width="0" layer="46" curve="-90"/>
<wire x1="21" y1="6" x2="11" y2="6" width="0" layer="46"/>
<wire x1="11" y1="6" x2="10" y2="7" width="0" layer="46" curve="-90"/>
<wire x1="10" y1="7" x2="10" y2="17" width="0" layer="46"/>
<wire x1="10" y1="17" x2="11" y2="18" width="0" layer="46" curve="-90"/>
</plain>
<libraries>
<library name="FlashPCB_Hardware">
<packages>
<package name="MOUNT-HOLE-M3">
</package>
</packages>
</library>
<library name="FlashPCB_Logos">
<packages>
<package name="FLASHPCB-LOGO-POLY-HEIGHT-2_54MM">
<description>&lt;b&gt;FlashPCB Logo &lt;/b&gt; - 2.540 x 19.258 mm / 0.100 x 0.758 in</description>
</package>
<package name="NONE">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MH1" library="FlashPCB_Hardware" package="MOUNT-HOLE-M3" value="MOUNT-HOLE-M3M3"/>
<element name="MH2" library="FlashPCB_Hardware" package="MOUNT-HOLE-M3" value="MOUNT-HOLE-M3M3"/>
<element name="MH3" library="FlashPCB_Hardware" package="MOUNT-HOLE-M3" value="MOUNT-HOLE-M3M3"/>
<element name="MH4" library="FlashPCB_Hardware" package="MOUNT-HOLE-M3" value="MOUNT-HOLE-M3M3"/>
<element name="U$1" library="FlashPCB_Logos" package="FLASHPCB-LOGO-POLY-HEIGHT-2_54MM" value=""/>
<element name="U$3" library="FlashPCB_Logos" package="FLASHPCB-LOGO-POLY-HEIGHT-2_54MM" value=""/>
<element name="LOGO1" library="FlashPCB_Logos" package="NONE" value="SCH-FLASHPCB-LOGO-WIRE-HEIGHT-8_89MM"/>
</elements>
<signals>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
</signals>
</board>
</drawing>
</eagle>
