<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="10" width="0" layer="20"/>
<wire x1="0" y1="10" x2="38" y2="10" width="0" layer="20"/>
<wire x1="38" y1="10" x2="38" y2="0" width="0" layer="20"/>
<wire x1="38" y1="0" x2="0" y2="0" width="0" layer="20"/>
<text>1.0mm</text>
<text>0.9mm</text>
<text>0.8mm</text>
<text>0.7mm</text>
<text>0.6mm</text>
<text>0.5mm</text>
<text>0.4mm</text>
<text>0.3mm</text>
<text>0.2mm</text>
<text>Soldermask
Limit Demo</text>
<text>Soldermask
Limit Demo</text>
<text>To adjust which vias are covered by soldermask change the mask limit in DRC --&gt; Masks --&gt; Limit</text>
</plain>
<libraries>
<library name="FlashPCB_Logos">
<packages>
<package name="NONE">
</package>
<package name="FLASHPCB-LOGO-WIRE-HEIGHT-2_03MM">
<description>&lt;b&gt;FlashPCB Logo &lt;/b&gt; - 2.032 x 15.407 mm / 0.080 x 0.607 in</description>
</package>
</packages>
</library>
<library name="FlashPCB_Hardware">
<packages>
<package name="MOUNT-HOLE-#4-PTH">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LOGO1" library="FlashPCB_Logos" package="NONE" value="SCH-FLASHPCB-LOGO-WIRE-HEIGHT-8_89MM"/>
<element name="MH1" library="FlashPCB_Hardware" package="MOUNT-HOLE-#4-PTH" value="MOUNT-HOLE-#4-PTH#4-PTH"/>
<element name="MH2" library="FlashPCB_Hardware" package="MOUNT-HOLE-#4-PTH" value="MOUNT-HOLE-#4-PTH#4-PTH"/>
<element name="U$1" library="FlashPCB_Logos" package="FLASHPCB-LOGO-WIRE-HEIGHT-2_03MM" value=""/>
<element name="U$2" library="FlashPCB_Logos" package="FLASHPCB-LOGO-WIRE-HEIGHT-2_03MM" value=""/>
</elements>
<signals>
<signal name="TOP">
<contactref element="MH1" pad="P$1"/>
</signal>
<signal name="BOTTOM">
<contactref element="MH2" pad="P$1"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
